# Instruction manual No.16

# C:\Users\PC\Desktop\jvdw90.png

SECOND HAND OF THE CHRONOGRAPH

MINUTE HAND

BUTTON A

HOUR HAND

24-HOUR HAND

POSITION 1

MINUTE HAND OF THE CHRONOGRAPH

POSITION 2

CROWN IN INITIAL POSITION

BUTTON B

SECOND HAND

**Instruction manual:**

**Time setting:**

1. Pull crown out to position 2.
2. Turn crown to advance hour and minute hands.
3. Push crown back to initial position. Second hand starts moving.

**Date setting:**

1. Pull crown out to position 1.
2. Turn crown counterclockwise to set the correct date. Do not set the date between 09:00 PM and 01:00 AM – the date would not change on the next day.
3. Push crown back to initial position.

**Using chronograph:**

Chronograph’s function is time tracking. It measures time in 1/1 seconds. The maximal amount of time it can measure is 59 minutes and 59 seconds. After start, the chronograph will measure and show time until it reaches the maximal amount of time.

1. Press button A to start/stop chronograph.
2. Press button B to reset chronograph. All hands will return to initial position.



**Resetting chronograph** (e.g. after battery replacement)

Follow these instructions if the second hand of the stopwatch does not return to 00:00 after the reset or after battery replacement.

1. Pull crown out to position 2.
2. Press button A to set second hand of the stopwatch to position 00:00. You can speed up the process by holding button A.
3. When the second hand is at 00:00, push crown back to initial position.

Attention: Do not push crown back to initial position before second hand reaches 00:00. If you did so, you would set this point as the new initial point.

